IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView]"
Time stamp: "2020-11-10T17:04:25"
Author: "NBS"
Preprocessor: "Xbim.Ifc File Processor version 2.4.1.0"
Originating system: "Xbim version 2.4.1.0"
Authorization: "Add company name here"
Application: "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS"

People and organizations
  Person "NBS" of Organization "Add company name here"
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change ADDED | created 1605027865 (2020-11-10T17:04:25Z)
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change MODIFIED | created 1605027865 (2020-11-10T17:04:25Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Add company name here"
  IFCSITE "Default site"
    IFCBUILDING "Default building"
      contains 1 element
        1 x IFCSLAB | type IFCSLABTYPE "NBS_JutaUKLtd_PlasticsSheets_JUTAGPTitanTank" | FLOOR | names: "NBS_JutaUKLtd_PlasticsSheets_JUTAGPTitanTank" | material: layers "NBS_JutaUKLtd_PlasticsSheets_JUTAGPTitanTank" ("NBS_JutaUKLtd_PlasticsSheets_JUTAGPTitanTank" 1.2) | property sets: COBie

Types
  IFCSLABTYPE "NBS_JutaUKLtd_PlasticsSheets_JUTAGPTitanTank" | FLOOR | 1 occurrence | material: layers "NBS_JutaUKLtd_PlasticsSheets_JUTAGPTitanTank" ("NBS_JutaUKLtd_PlasticsSheets_JUTAGPTitanTank" 1.2) | property sets: xbim_MaterialFunctionAssignment, COBie, Pset_CoveringCommon, BOS_General, NBS_Data

Property sets
  COBie | properties | on 1 object (1 IFCSLAB)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_57_65_60:Plastics sheets" (IFCTEXT)
    CodePerformance = "BS 8485:2015, BS 8102:2009" (IFCTEXT)
    Color = "Black" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Self-adhesive version of GP Titanflex" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Sustainable and innovative multi-function barrier membrane with industry leading performance" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "info@juta.co.uk" (IFCTEXT)
    Material = "Multi Layer Polyethelene" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "JUTA GP TitanTank" (IFCTEXT)
    Name = "PlasticsSheets_JUTAGPTitanTank_JutaUKLtd" (IFCTEXT)
    NominalHeight = 1.2 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 20000. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Flat sheet applied - supplied in roll form" (IFCTEXT)
    Size = "20000 x 1000 x 1.2 mm" (IFCTEXT)
    SustainabilityPerformance = "LEED Certified Product" (IFCTEXT)
    WarrantyDescription = "120 Year Product Warranty" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  xbim_MaterialFunctionAssignment | properties | on 1 type object
    MaterialFunctionAssignment (ifcpropertytablevalue)
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "Smooth" (IFCTEXT)
    FireRating = "EN 13501-1 Class E" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "Non-Fragile" (IFCTEXT)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "n/a" (IFCTEXT)
    Status = "UNSET" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    ThermalTransmittance = 0. (IFCREAL)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_JutaUKLtd_PlasticsSheets_JUTAGPTitanTank" (IFCTEXT)
    ManufacturerName = "Juta UK Ltd" (IFCTEXT)
    ManufacturerURL = "www.juta.co.uk" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/gdg5pngr" (IFCTEXT)
    NBSDescription = "Plastics sheets" (IFCTEXT)
    NBSReference = "45-65-50/325" (IFCTEXT)
    ProductInformation = "https://www.juta.co.uk/gas-protection-membranes/voc-hydrocarbon-membranes/gp-titantank/" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_57_65_60" (IFCTEXT)
    Uniclass2015Title = "Plastics sheets" (IFCTEXT)
    Uniclass2015Version = "Products v1.20" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    Form = "Post Applied Self-Adhesive VOC/ Hydrocarbon and Waterproofing Barrier Membrane" (IFCTEXT)
    PerformanceAntistaticProperties = "n/a" (IFCTEXT)
    PerformanceColour = "Black" (IFCTEXT)
    PerformanceElongationToBreak = ">550 %" (IFCTEXT)
    PerformanceFirePerformance = "EN 13501-1 Class E" (IFCTEXT)
    PerformanceResistantToUndergroundGases = "Methane - 0.13 ml/m²/day atm. Carbon Dioxide - 3.01 ml/m²/day/atm. Radon - 1.0 x 10(-12). Vinyl Chloride - 0.04 ml/m²/day/atm" (IFCTEXT)
    PerformanceTearResistance = ">300 N" (IFCTEXT)
    PerformanceTensileStrengthMinimum = ">400 N/ 50 mm" (IFCTEXT)
    PerformanceUvStabilization = "To be covered within one month of application" (IFCTEXT)
    PerformanceWaterVapourResistanceMinimum = "0.11 G/ M²/ Day" (IFCTEXT)
    PhysicalPropertiesDimensionsRollLengthMinimum = "20 M" (IFCTEXT)
    PhysicalPropertiesDimensionsThicknessMinimum = "1.2 mm" (IFCTEXT)
    PhysicalPropertiesDimensionsWidthMinimum = "0.3 M" (IFCTEXT)
    PhysicalPropertiesWeightMinimum = "1350 G/ M²" (IFCTEXT)
    Purpose = "For the gas/ waterproofing, tanking of underground structures where harmful ground gases are anticipated" (IFCTEXT)
    RecycledContent = "0" (IFCTEXT)
    RootInhibitor = "Yes - Tested to CEN/TS 14461" (IFCTEXT)
    Standard = "BS 8485:2015, BS 8102:2009, CIRIA C748, CIRIA C735" (IFCTEXT)
    ThirdPartyCertification = "CE Mark: EN13967:2012, BBA Certificate 18/5581" (IFCTEXT)